../HW_Devices/rs522.c:18:9:ReadRawRC	24	static
../HW_Devices/rs522.c:38:6:WriteRawRC	24	static
../HW_Devices/rs522.c:56:6:SetBitMask	24	static
../HW_Devices/rs522.c:71:6:ClearBitMask	24	static
../HW_Devices/rs522.c:86:6:PcdAntennaOn	16	static
../HW_Devices/rs522.c:104:6:PcdAntennaOff	8	static
../HW_Devices/rs522.c:118:6:PcdReset	8	static
../HW_Devices/rs522.c:140:6:M500PcdConfigISOType	16	static
../HW_Devices/rs522.c:171:6:PcdComMF522	48	static
../HW_Devices/rs522.c:282:6:PcdRequest	48	static
../HW_Devices/rs522.c:314:6:PcdAnticoll	56	static
../HW_Devices/rs522.c:353:6:CalulateCRC	40	static
../HW_Devices/rs522.c:383:6:PcdSelect	48	static
../HW_Devices/rs522.c:426:6:PcdAuthState	56	static
../HW_Devices/rs522.c:465:6:PcdWrite	48	static
../HW_Devices/rs522.c:506:6:PcdRead	48	static
../HW_Devices/rs522.c:539:6:PcdHalt	40	static
../HW_Devices/rs522.c:552:6:IC_CMT	32	static
../HW_Devices/rs522.c:571:6:RC522_Init	8	static
