(footprint "EC11" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 622F3FAB)
  (attr through_hole)
  (fp_text reference "SW**" (at -5.08 -12.08 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5641be26-f5e9-482f-8616-297f17f4eae2)
  )
  (fp_text value "EC11" (at -5.08 -10.58 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 90d503cf-92b2-4120-a4b0-03a2eddde893)
  )
  (fp_text user "${REFERENCE}" (at -5.08 -9.08 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 86143bb0-7899-4df8-b1df-baa3c0ac7889)
  )
  (fp_line (start -5.9 6.3) (end -5.9 -5.7) (layer "F.SilkS") (width 0.12) (tstamp 96ee9b8e-4543-4639-b9ea-44b8baaaf94e))
  (fp_line (start 5.8 6.3) (end -5.9 6.3) (layer "F.SilkS") (width 0.12) (tstamp a819bf9a-0c8b-443a-b488-e5f1395d77ad))
  (fp_line (start -5.9 -5.7) (end 5.8 -5.7) (layer "F.SilkS") (width 0.12) (tstamp ac8576da-4e00-41a0-9609-eb655e96e10b))
  (fp_line (start 5.8 -5.7) (end 5.8 6.3) (layer "F.SilkS") (width 0.12) (tstamp b83b087e-7ec9-44e7-a1c9-81d5d26bbf79))
  (pad "6" thru_hole rect (at -6.25 0) (size 1.5 2.5) (drill oval 1 2.2) (layers *.Cu *.Mask) (tstamp 28d267fd-6d61-43bb-9705-8d59d7a44e81))
  (pad "7" thru_hole rect (at 6.25 0) (size 1.5 2.5) (drill oval 1 2.2) (layers *.Cu *.Mask) (tstamp 848901d5-fdee-4920-a04d-fbc03c912e79))
  (pad "A" thru_hole circle (at -2.5 7.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask) (tstamp dfba7148-cad3-4f40-9835-b1394bd30a2c))
  (pad "B" thru_hole circle (at 2.5 7.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask) (tstamp 92d17eb0-c75d-48d9-ae9e-ea0c7f723be4))
  (pad "C" thru_hole circle (at 0 7.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask) (tstamp c2211bf7-6ed0-4800-9f21-d6a078bedba2))
  (pad "S1" thru_hole rect (at -2.5 -7) (size 2 2) (drill 1.2) (layers *.Cu *.Mask) (tstamp f8a90052-1a8b-4ce5-a1fd-87db944dceac))
  (pad "S2" thru_hole circle (at 2.5 -7) (size 2 2) (drill 1.2) (layers *.Cu *.Mask) (tstamp fab985e9-e679-4dd8-a59c-e3195d08506a))
)
