(footprint "OLED12864" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62311A46)
  (attr through_hole)
  (fp_text reference "Dis**" (at -5.5 -6.3 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4c9fdea7-ba0c-45cc-8f66-240980c37d5c)
  )
  (fp_text value "OLED12864" (at -5.5 -4.8 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c58960d9-4cac-4036-ad2e-1aef26946dae)
  )
  (fp_text user "${REFERENCE}" (at -5.5 -3.3 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5b96c1ad-46ba-4366-8241-fbc1cd0e9bbd)
  )
  (fp_line (start 26 20) (end 3 20) (layer "F.SilkS") (width 0.12) (tstamp 0ce8d3ab-2662-4158-8a2a-18b782908fc5))
  (fp_line (start 0 28) (end 28 28) (layer "F.SilkS") (width 0.12) (tstamp 213a2af1-412b-47f4-ab3b-c5f43b6be7a6))
  (fp_line (start 26 3) (end 26 20) (layer "F.SilkS") (width 0.12) (tstamp 27d56953-c620-4d5b-9c1c-e48bc3d9684a))
  (fp_line (start 28 0) (end 0 0) (layer "F.SilkS") (width 0.12) (tstamp 34871042-9d5c-4e29-abdd-a168368c3c22))
  (fp_line (start 2 3) (end 26 3) (layer "F.SilkS") (width 0.12) (tstamp 82be7aae-5d06-4178-8c3e-98760c41b054))
  (fp_line (start 2 20) (end 2 3) (layer "F.SilkS") (width 0.12) (tstamp 89e83c2e-e90a-4a50-b278-880bac0cfb49))
  (fp_line (start 3 20) (end 2 20) (layer "F.SilkS") (width 0.12) (tstamp 8c0807a7-765b-4fa5-baaa-e09a2b610e6b))
  (fp_line (start 28 28) (end 28 0) (layer "F.SilkS") (width 0.12) (tstamp 9702d639-3b1f-4825-8985-b32b9008503d))
  (fp_line (start 0 0) (end 0 28) (layer "F.SilkS") (width 0.12) (tstamp f144a97d-c3f0-423f-b0a9-3f7dbc42478b))
  (pad "1" thru_hole rect (at 10.2 0.9) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask) (tstamp 2732632c-4768-42b6-bf7f-14643424019e))
  (pad "2" thru_hole circle (at 12.74 0.9) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask) (tstamp 120a7b0f-ddfd-4447-85c1-35665465acdb))
  (pad "3" thru_hole circle (at 15.28 0.9) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask) (tstamp e877bf4a-4210-4bd3-b7b0-806eb4affc5b))
  (pad "4" thru_hole circle (at 17.82 0.9) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask) (tstamp 5b2b5c7d-f943-4634-9f0a-e9561705c49d))
)
